1. Check diode polarity is shown on Silkscreens of TOP and BOTTOM.
2. Check polarity of tantalum and electrolytic capacitor should be soldered correctly.
3. Check pin no 1 of connector should be soldered on pin 1 on footprint in PCB.
4. Check that Glue to be used every time where wire is soldered on board.
5. Check anti corrosive spray is applied.
6. Refer TOP & BOTTOM Silkscreen Given below.



