**Features:**

1. On board AC to DC converter.
2. Cut-off relay is available.
3. Sensor can be interfaced on board.

**Technical Specification:**

1. Power Supply: AC 220V/110V.
2. Product designed meets IP 65 standards.
3. Operating tempt: 0°C to 60°C.
4. Storage tempt: 0°C to 80°C.
5. PCB Size: 90mm X63mm.
6. No. of Layer: Single Layer.