|  |  |
| --- | --- |
| Working Voltage Range | +9V to +24V DC |
| Current Consumption DC (mA) | 37.47 mA(Max) @24VDC |
| Power Consumption | 0.8992W(Max) @ 24VDC |
| Operating temperature | 0°C to+ 60°C |
| Storage temperature | -20°C to +80°C |
| PCB size | 160 mm X 100 mm |
| List of Components (IC) | 1. PIC18F25K80 (MICRO-CONTROLLER) 2. MC33972 (INPUT IC) 3. MC33996 (OUTPUT IC) 4. BT 832X (NRF) 5. MAX 232 (RS 232 IC) 6. MCP 2551 (CAN IC) 7. LM2576 (5V VOLTAGE REGULATOR) 8. LD1117CTR (3.3 V VOLTAGE REGULATOR) |